EFIS Control Panel

This instrument lets you control the Navigation Display.

| The Visibility Buttons will show or hide elements displayed on the ND. They are very useful when you fly in a region with many navaids, it allows you to keep a clear display. CSTR shows/hides the route entered in the FMGC WPT shows/hides intersections (also called waypoints) VORD shows/hides VOR stations NDB shows/hides NDB stations ARPT shows/hides airports The left rotating button lets you select the ND mode. Read the ND section for more information about each mode. The right button is for range selection. Navaid 1 and Navaid 2 are 3-state switches. They can be switched on the ADF, OFF or VOR position. If ADF is selected on one of the switches, the ADF needle will be displayed on the ND. Only one ADF is available in FS2002. If VOR is selected, the corresponding VOR needle (VOR1 for navaid 1 switch, VOR2 for navaid 2) will be displayed on the ND. If OFF is selected, no needle is displayed for the corresponding navaid on the ND, and "----" is displayed instead of the navaid name. This is useful when you want to have a clear display, especially on final approach when you only need to visualize the ILS information.

Continue to the FCU page